**O Ring Size chart for O-ring store**

|  |  |  |  |
| --- | --- | --- | --- |
| **Actual Size** | **Size** | **Database Reference** | **Typical Use** |
|  | BS003 | rgp10 | High-Pressure Hose/SPG swivel |
|  | BS004 | or002 | Some HP swivels |
|  | BS006 | or003 | BC power inflate |
|  | BS010 | rgp13 | Low-Pressure Hose/2nd Stage, Regulator Cylinder Valve Stem |
|  | BS011 | rgp11 | Standard Low-Pressure Port/Hose (3/8 UNF) |
|  | BS012 | rgp12 | High-Pressure Port/Hose (7/16 UNF), Manifold and Manifold Port Plugs |
|  | BS013 | or007 | Large Low-Pressure Port/Hose (1/2 UNF) |
|  | BS014 | cpp23 | Standard Yoke Regulator/K-valve |
|  | BS015 | or009 | Cylinder Valve Bonnet Nut |
|  | BS110 | or010 | MDE Yoke Valves |
|  | BS111 | or011 | Small DIN Regulator/Valve |
|  | BS112 | or012 | Standard DIN Regulator/Valve (Nearly all DIN regulators) |
|  | BS116 | or013 | Cylinder with Small Neck/Valve (7/8 UNF - "Genesis" 3500 psi Steel cylinders) |
|  | BS210 | or014 | BC dump valves |
|  | BS214 | or015 | Cylinder with Large Neck/Valve (3/4 NPS - All Aluminium, most Steel cylinders) |